Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 67 - Abbott
P. 67

    The system should not be modified. The user of this equipment is responsible for reading, understanding, and following the Warning
                    and Precaution statements presented within this manual.
                    Electromagnetic Interference and Electromagnetic Compatibility

                    This section provides a brief overview of Electromagnetic Interference and Electromagnetic Compatibility guidance associated with
                    the use of the CM3000.

                    Table 15.  Electromagnetic Emissions
                    Guidance and manufacturer’s declaration – electromagnetic emissions
                    The electronics unit is intended for use in the electromagnetic environment specified below.
                    The customer or the user of the electronics unit should assure that it is used in such an environment.

                    Emissions test                Compliance                     Electromagnetic environment -
                                                                                 guidance
                    RF emissions                                                 The electronics unit must emit
                    CISPR 11                      Class A, Group 2               electromagnetic energy in order to perform
                    CISPR 22                      Class B                        its intended function. Nearby electronic
                    Harmonic emissions            Class A                        equipment may be affected.
                    IEC 61000-3-2                                                The electronics unit is suitable for use in
                                                                                 all establishments, including domestic
                    Voltage fluctuations/         Complies                       establishments and those directly
                    Flicker emissions                                            connected to the public low-voltage power
                    IEC 61000-3-3                                                supply network that supplies buildings
                                                                                 used for domestic purposes.

                    Table 16.  Electromagnetic Immunity
                    Guidance and manufacturer’s declaration – electromagnetic immunity
                    The electronics unit is intended for use in the electromagnetic environment specified below. The customer or the user of the
                    electronics unit should assure that it is used in such an environment.
                    Immunity Test    IEC 60601          Compliance level   Electromagnetic environment - guidance
                                     Test level
                    Electrostatic discharge  ±8 kV contact   ±8 kV contact   Floors should be wood, concrete or ceramic tile. If
                    (ESD)            ±15 kV air         ±15 kV air         floors are covered with synthetic material, the
                    IEC 61000-4-2                                          relative humidity should be at least 30%.
                    Electrical fast   ±2 kV for power supply   ±2 kV for power supply   Mains power quality should be that of a typical
                    transient/burst   lines             lines              commercial or hospital environment
                    IEC 61000-4-4    ±1 kV for input/output   ±1 kV for input/output
                                     lines              lines
                    Surge            ±1 kV line(s) to line(s)   ±1 kV line(s) to line(s)   Mains power quality should be that of a typical
                    IEC 61000-4-5    ±2 kV line(s) to earth   Not applicable   commercial or hospital environment
                    Voltage dips, short   0% UT  (100% dip in   0% UT (100% dip in UT)   Mains power should be that of a typical
                                         15
                    interruptions and   UT) for 0.5 cycle   for 0.5 cycle   commercial or hospital environment. If the user of
                    voltage variations on   0% UT (100% dip in UT)   0% UT (100% dip in UT)   the electronics unit requires continued operation
                    power supply input   for 1 cycle    for 1 cycle        during power mains interruptions, it is
                    lines                                                  recommended that the electronics unit be
                    IEC 61000-4-11   70% UT (30% dip in UT)   70% UT (30% dip in UT)   powered from an uninterruptible power supply or a
                                     for 25 cycles      for 25 cycles      battery.
                                     0% UT (100% dip in UT)   0% UT (100% dip in UT)
                                     for 5 sec          for 5 sec
                    Power frequency   30 A/m            30 A/m             Power frequency magnetic fields should be at
                    (50/60 Hz)                                             levels characteristic of a typical location in a
                    Magnetic field                                         typical commercial or hospital environment.
                    IEC 61000-4-8
                    Conducted RF     3 Vrms             3 Vrms             Portable and mobile RF communication
                    IEC 61000-4-6    150 kHz to 80 MHz                     equipment should be no closer to any part of the
                                     ISM Bands          6 Vrms             electronics unit, including cables, than the
                    Radiated RF      3 V/m              3 V/m              recommended separation distance calculated
                    IEC 61000-4-3    80 MHz to 2.7 GHz                     from the equation applicable to the frequency of

                    15  UT is the a.c. mains voltage level prior to application of the test level.

                                                                63

| 62 63 64 65 66 67 68 69 70 71 72 |