Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 70 - Abbott
P. 70

    Environmental Information
                      Operation: 5º to 40ºC (41º to 104ºF), 15% to 93% humidity (non-condensing), 700-1060 hPa (Electronics), 800-1150 hPa
                       (implanted sensor)
                      Transportation: -25º to 70ºC (-13º to 158ºF) and up to 93% humidity (non-condensing)
                      Storage: -25º to 70ºC (-13º to 158ºF) and up to 93% humidity (non-condensing)
                   Classification
                      Class II equipment
                      Type BF insulation
                      Ordinary Equipment IP 21
                      Continuous Use

                   Testing
                   System Testing
                      System Accuracy (under typical environmental conditions): +/- 2 mmHg at baseline and +/-3% of difference between measured
                       pressure and baseline
                      System Accuracy: +/-4 mmHg over the range of environmental conditions
                      The CM3000 was issued an ETL/cETL Listing Mark
                   Safety Testing
                      IEC 60601-1
                      ANSI ES 60601-1
                      CENELEC EN 60601-1
                      CAN/CSA-C22.2 No. 60601-1
                   EMI/EMC Testing
                      CENELEC EN 60601-1-2
                      ETSI EN 301 489-1
                   Wireless Testing
                      FCC part 18 (Electronics System)
                      FCC part 15 (Sensor)
                      ETSI EN 301 489-3
                      ETSI EN 302 510
                      CISPR 11
                      CISPR 22
                   Software

                   This device contains open source software. Source code is available upon request.
                   Technical Support
                   In North America:
                   For Merlin.net™ PCN patients, telephone Technical Support is available Monday through Friday (8AM to 8PM Eastern Standard
                   Time). For clinicians, telephone Technical Support is available 24-hours a day.
                   For Merlin.net Patient Care Network support:
                      1 877 696 3754 (1 877 MY MERLIN) (toll-free within North America)
                   In Europe:
                   Telephone Technical Support is available Monday through Friday (8:00 to 17:00 Central European Time).
                      +46 8 474 4756 (Sweden) (Support in English and Swedish)
                   St. Jude Medical maintains 24-hour phone lines for technical questions and support:
                      1 818 362 6822
                      1 800 722 3774 (toll-free within North America)
                      + 46 8 474 4147 (Sweden)
                   For additional assistance, call your local St. Jude Medical representative.
                   Symbols
                   The following symbols are used on the system labels.
                   Symbol            Description
                                     Reorder number

                                                                66

| 65 66 67 68 69 70 71 72 73 74 75 |