Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 6 - Abbott
P. 6

       All sensors have a unique calibration. Ensure readings are only taken using the correct calibration information from the sensor.
                       Use of the incorrect calibration information may result in an inaccurate reading.
                      All right heart catheterizations must be performed under fluoroscopic guidance to prevent sensor dislodgement.
                      The sensor is visible under plain film X-ray and fluoroscopy. Under CT imaging, there may be localized beam hardening artifact
                       around sensor implant.
                      This product is not made with natural rubber latex.
                   Precautions
                      Store the CM3000 in a temperature controlled, clean and dry area.
                      Use the CM3000 at temperatures between 5º to 40ºC (41º to 104ºF) and 15% to 93% humidity. Store the system between -25
                       to 70ºC (-13º to 158ºF) and up to 93% humidity.
                      All electronic devices with the Hospital and Patient Electronics Systems, including components and accessories, are to be used
                       only with the sensor and not with other products, appliances or devices. If there is evidence of a change in performance, please
                       contact Technical Support to obtain more information.
                      Avoid excessive or damaging force when using the AC adapter.
                      Exposure to excess lint or dust may cause the system to malfunction.
                      The system consists of an electronics unit and an antenna. If any of the following occurs, immediately unplug the electronics
                       unit and contact Technical Support:
                       -   Any cords are noticeably frayed or damaged
                       -   Liquid has spilled onto the monitor, or it has been exposed to rain
                       -   The system has been dropped or the enclosure has been damaged
                      If you lose the power cord, replace it with an identical cord. Contact Technical Support to obtain a new one.
                      Only an authorized technician should remove the cover or attempt to service the device. The warranty may be voided otherwise.
                      Do not place the system near a window. Exposing the LCD screen to rain, water, moisture or sunlight may severely damage it.
                      Do not apply excessive pressure to the LCD screen. Excessive pressure may cause damage to the display.
                      Portable and mobile RF communications equipment can affect medical electrical equipment and may cause a malfunction of
                       the system.
                      All new or refurbished equipment should be obtained from the manufacturer.
                      The CM3000 may require secure data transfer through the use of the internet or networks. Portions of this internet or network
                       pathway may become unavailable for periods of time for a variety of reasons including but not limited to: internet connectivity
                       outage, hardware failure, power outage, or general infrastructure failures. Readings and data that are unable to transmit are
                       stored and will transmit when connectivity is available.
                      The mean pressure measurement accuracy of the system may be affected by various factors. Mean pressure measurement
                       error has been observed when the sensor was deployed in a vessel which had an inner diameter of less than 7 mm, and in
                       cases where there was an acute bend in the vessel of >30 degrees at the location of the sensor. Signs of mean pressure
                       measurement error include the following:
                       -   Gradual mean pressure changes without a corresponding proportional change in the pulse pressure (systolic-diastolic
                           pressure)
                       -   Negative mean pressures
                       If either feature is observed, temporarily suspend use of the pressure information for management of the patient and contact
                       Technical Support for further assistance. A right heart catheterization may be needed to recalibrate the Baseline (mean
                       pressure) in order to continue use of the system.
                      The touchscreen display on the handheld unit can be sensitive to electrostatic discharge (ESD) at high levels. To reduce the
                       potential for ESD discharge to the touchscreen, remove and hold the plastic handle of the handheld prior to contact with the
                       touchscreen.
                       If the touchscreen becomes damaged due to ESD, the screen will be discolored or may be unresponsive. Contact Technical
                       Support for replacement of the handheld unit.
                       Please note that high levels of ESD are more likely in situations where the relative humidity is very low, such as inside a heated
                       building during the winter in areas where it is cold outside. In order to reduce the potential for ESD levels, there are common
                       situations which create static electricity that can be avoided prior to use, for example, putting on and removing clothes,
                       dragging your feet across a carpet or rug, vacuuming, or removing clothes from a dryer.
                      The system is not intended to be used in a severe electromagnetic radiation environment or an industrial environment.
                      The system should not be used in conjunction or in association with Magnetic Resonance Imaging (MRI), computerized axial
                       tomography (CT), diathermy, Radio Frequency Identification (RFID), and electromagnetic security systems such as metal
                       detectors.
                   Package Contents

                   The system package contains:
                      Hospital Electronics System
                      Product documentation

                                                                2

| 1 2 3 4 5 6 7 8 9 10 11 |