Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 7 - Abbott
P. 7

    Sterilization

                    The Hospital Electronics System is provided non-sterile.
                    Components and Setup

                    Connect the System Cables
                    1.   Align the keyed antenna at an approximately 30 degree angle and twist on the locking connector.

                    Figure 1.  Connecting the antenna

                    2.   Attach the connectors as shown in the figure below.
                       Connectors:
                       -   Power supply connector (5 pin DIN)
                       -   Printer serial communication cable (9 pin D-SUB )
                       -   Printer power cable
                       Note: A VGA cable can be connected to the auxiliary VGA connector.

                    Figure 2.  The connectors
                                                                       1.  Power switch
                                                                       2.  Power cable
                                                                       3.  Printer serial cable
                                                                       4.  VGA connection
                                                                       5.  Printer power cable

                    3.   Plug the power cord into the power supply and plug the power cord into the wall.
                    Printer
                    The printer clips into the mount on the front of the electronics unit. The cables for the printer run under the electronics unit.
                    Disconnect them if necessary.

                                                                3

| 2 3 4 5 6 7 8 9 10 11 12 |