Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 69 - Abbott
P. 69

    FCC Statement

                    This device complies with Part 18 of the FCC rules.
                    The PA Sensor is approved for wireless transmission under FCC ID number R3PCS-A-000051. The sensor complies with Part 15 of
                    the FCC Rules. Operation is subject to the following two conditions: 1) this device may not cause harmful interference and 2) this
                    device must accept any interference received, including interference that may cause undesired operation.
                    EU REACH SVHC Disclosure

                    Current Candidate List (as published July 2014)
                    REACH - the regulation concerning Registration, Evaluation, Authorization and Restriction of Chemicals - is a law within the
                    European Union. REACH applies to all EU manufacturers, importers and users of chemical substances, as well as EU producers,
                    importers and suppliers of articles such as finished goods, parts and components.
                    Article 33 of REACH requires us to provide information about certain “substances of very high concern” (“SVHCs”) if any SVHCs are
                    present in a concentration of more than 0.1% of the weight of an article that we supply in the EU.
                    Based on information currently available, no substances from the SVHC candidate list are present in our products as described by
                    Article 33, except as follows:
                    (DEHP, bis(2-ethyl(hexyl)phthalate), CAS nr.: 117-81-7; EC nr. 204-211-0).
                    DEHP is found in the following component(s):

                    Table 18.  Component
                    Component               Part                     Amount Present
                    Rigid Antenna           CS-000132                Less than 0.8% w/w (weight of substance/weight of
                                                                     product)

                    As a result, there are no restrictions for the user of the rigid antenna in this application.
                    WEEE Compliance Statement
                    The 2002/96/EC Directive on Waste Electrical and Electronic Equipment (the WEEE Directive) states that new equipment placed on
                    the market within the European Union must comply with the WEEE directive which aims to ensure that products can be easily
                    broken down or recycled at the end of the life cycle. The manufacturer is committed to complying with the EC WEEE directive.
                    Products put on the market are required to be marked with the crossed through recycling bin symbol and something that identifies
                    that it was put on the market on or after this date.
                    System Specifications

                    Electrical Characteristics
                    Power
                       Power Supply: Input: Class II 100-240V, 50-60 Hz, Output: 12 VDC, 6A
                       Manufacturer part number: CS-001301
                       Only use power cord (CM3020) supplied by the manufacturer
                    Radiofrequency (RF) Characteristics
                       Transmitted Electrical Power: < 1 mW e.r.p.
                       Operating Frequency:  30-37.5 MHz. Under normal operating conditions the measurement bandwidth is approximately 1 MHz
                       within the operating frequency range.
                    Mechanical Characteristics
                    Main Unit
                       Weight: approximately 8 pounds
                       Dimensions: Height:11.5 inches Width: 10.5 inches Length: 5.5 inches
                       Product Life: 5 years
                       I/O: 2 USB, RS-232
                       Printer: FP-900064
                       Optional WIFI adapter: CM3040
                    Display
                       Touchscreen: Resistive
                       Brightness: approximately 250 cd/m2
                       Resolution: 800 x 480, color
                    Antenna
                       Weight: approximately 4 pounds
                       Diameter: 9 inches
                       Cable: Reference manufacturer’s part number CS-000135

                                                                65

| 64 65 66 67 68 69 70 71 72 73 74 |