Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 43 - Abbott
P. 43

    WiFi is not installed by default. Contact Customer Service to obtain the compatible WiFi accessory.
                    Once you have obtained the WiFi accessory, contact the IT group at your facility for credentials to your WiFi network. Some important
                    information to consider regarding the use of WiFi by the Hospital Electronics System.
                       The system only uses the WiFi network at your facility as a means to gain access to the Merlin.net Patient Care Network Heart
                       Failure Management Application which is available on the internet.
                       The system does not communicate with any other devices within your facilities’ network.
                       All information passed between the system and the Merlin.net Patient Care Network Heart Failure Management Application is
                       encrypted using secure sockets (SSL).
                       The system will only operate on WiFi networks that are sufficiently encrypted (WPA2). It will not operate on unprotected or open
                       networks.
                       The credentials for the WiFi network are not sent to the Merlin.net Patient Care Network Heart Failure Management Application.
                    Using the screen below, enable the network and then enter the network name and password.

                    Figure 74.  WiFi Setup

                    B. Setting Baseline in Follow-Up Reading
                    If the follow-up readings are being performed in the cardiac catheterization lab, you will be able to set the baseline to a new value.
                    1.   Select the Baseline button at the top of the screen. This will enable the buttons used during implant to set the baselines.

                    Figure 75.  Setting Baseline in Follow-Up

                    2.   Select Set Pressure Baseline or Set CO Baseline to adjust baselines. Refer to the section Step 3: Set Baseline for instructions on
                       properly setting the baseline.
                    If there is any change to the baseline it is important to transfer the information back to the Merlin.net Patient Care Network Heart
                    Failure Management Application so that the system in your patient’s home uses the updated baseline.

                                                                39

| 38 39 40 41 42 43 44 45 46 47 48 |